**Title Page:**

Comparison of Novel Kalman Filter with Adaptive DWT Technique for Noise Detection and Removal in Real Time Images

K. Devendra1, Dr G.Kumaran2

K. Devendra1

Research Scholar,

Department of Computer Science and Engineering,

Saveetha School of Engineering,

Saveetha Institute of Medical and Technical Sciences,

Saveetha University, Chennai, Tamil Nadu, India, Pincode: 602105.

devandarak18@saveetha.com

Dr G.Kumaran2

Research Guide, Corresponding Author,

Department of Computer Science and Engineering,

Saveetha School of Engineering,

Saveetha Institute of Medical and Technical Sciences,

Saveetha University, Chennai, Tamil Nadu, India, Pincode: 602105.

[kumarang.sse@saveetha.com](mailto:kumarang.sse@saveetha.com)

**Keywords**: Real-time Images, Novel Kalman Filter, Adaptive discrete wavelet transform, Noise Detection Accuracy, Noise Removal, *Environment*

# **ABSTRACT**

**Aim:** The Primary task of this project work is to increase the accuracy of noise detection and noise removal in Real Time Images using the Novel Kalman Filter for Real Time findings and existing popular Adaptive DWT**. Materials and Methods:**The Novel Kalman Filter with a sample size of 110 and Adaptive DWTs with a g-power value of 0.8% are used in the suggested models to remove unwanted noise from Real Time Images. With the aid of the well-known Mean Filter from theMATLAB image processing package, the Real Time picture dataset is used for simulation. **Results and Discussion:** With the widely used Adaptive DWT, the accuracy of the results from the suggested Novel Kalman Filter is significantly increased (90.13% versus 89.35%). The suggested Novel Kalman Filter outperforms the Adaptive DWT in the area of Real Time image analysis, according to the accuracy values. The difference between the two groups is statistically significant, as shown by the p value of 0.005 (p 0.05). **Conclusion:** In terms of real-time picture assessments and results, the suggested research on Novel Kalman Filters implies that it is preferable than the Adaptive DWT currently in use.

**Keywords**: Real-time Images, Novel Kalman Filter, Adaptive discrete wavelet transform, Accuracy, Noise Elimination, *Environment*

**INTRODUCTION**

The new picture-handling procedures are utilized as a device to further develop identification abilities in clinical applications. Clinical pictures are impacted by various kinds of noises[(Zohreh HosseinKhani it all., 2017)](https://arxiv.org/ftp/arxiv/papers/1707/1707.05975.pdf).Picture denoising is the most common way of eliminating the noise from a picture. The expansion of noise will cause the loss of data. The noise can be started in numerous ways, for example, [(He et al. 2022)](https://paperpile.com/c/ihOtTi/f7Cl)while catching pictures in low-light circumstances, harm of electric circuits because of intensity, sensor enlightenment levels of a computerized camera or because of the broken memory areas in hardware or small errors in the transmission of information over significant distances [(Smolka and Chydzinski 2005)](https://paperpile.com/c/ihOtTi/3Doe) .Unwanted values of the pixel are added to the picture leading to losing the data. The Environment noise can be of different kinds like IN Impulse noise) in which the values of the pixel differ from the pixel values of the surrounding [(Ersboll 2007)](https://paperpile.com/c/ihOtTi/HhxT). There are two types that are RVIN and SPIN. In AWGN images will be altered from the exact value by a small amount. These algorithms are used in hill station,mountains .[(Philips, Popescu, and Scheunders 2007)](https://paperpile.com/c/ihOtTi/WPEf).

Elimination of Environment noise is a vital issue in the field of picture processing that has various removals of noise functions in many fields.[(Bouhlel and Rovetta 2019)](https://paperpile.com/c/ihOtTi/OCTe) Usually corrupting the noise of the image is impulsive in nature. Impulsive noise is very common which is caused by the malfunction of the hardware and other techniques of the image, transmission, or memory. These kinds of noise affect some of the individual pixels, altering the actual data.[(Marıa G. Sanchez et al., 2014)](https://reader.elsevier.com/reader/sd/pii/S1877050914003846?token=583B1EB870A05511C472387C39F19116C23A21123527BD4716AACCFBC201E604E109BAFA8309254344F2109811E02B1F&originRegion=eu-west-1&originCreation=20221017235306) Removal of noise is regularly finished with some straight or non-direct procedure on a bunch of nearby pixels and the relationship between the pixels accessible in the Spatio-temporal sense[(J. Li et al. 2019)](https://paperpile.com/c/ihOtTi/oUGh). The great video de-noising can be effectively accomplished by taking advantage of Environment Noise Elimination of data from both earlier edge and future methods[(S. Z. Li 2009)](https://paperpile.com/c/ihOtTi/8ZIF). Just hence, a considerable algorithm exploits data from normally the ongoing present edge and a couple of earlier frameworks.

Over the previous 5 years, nearly 300 research magazines were offered in GS (Google Scholar) and more than 150 papers existed in science direct journals with different types of filtering approaches. Compared to the outcome of the other types of filtering concepts, the Novel Kalman Filter eliminates the noises from the real-time images with a better accuracy rate. The main goal of this research study is to eliminate the Environment noises from real-time images using filtering concepts with better exactness.

**MATERIALS AND METHODS**

This current research process was designed and executed at the Image Processing Laboratory, Saveetha School of Engineering, SIMATS (Saveetha Institute of Real Time and Technical Sciences). The suggested noise elimination system contains two types of groups Group 1 is taken as Novel Kalman Filter and group 2 as Adaptive DWT. Novel Kalman Filter and Adaptive DWT were analyzed many times by 150 sample sizes. After the compilation of the real-time image database, repetitive and unimportant portions of the images were eliminated by filtering and data-cleaning processes. Then, it is related to the applicable data sets, and the accuracy rate of the Novel Kalman Filter and Adaptive DWT is calculated and compared.

**Novel Kalman Filter**

Filtering by the Kalman method is a framework that gives appraisals of a few unknown identifiers that provides the measurement of the estimations after some time. The filters of Kalman have been exhibiting their advantages in different fields. The filter of Kalman is very simple and needs less power of computation. Nonetheless, it is as yet difficult for individuals who do not know the estimation theory to progress the filtering process of Kalman. The filters of the Kalman algorithm comprise two phases: Detection and update. It is noted that "detection" and "update" are frequently called "propagation" and "correction," separately, in various literature**.**

**Pseudo code**

input-Coaching and data verification are inputs.

output-accuracy

1. First, load the dataset.

2: Data from the dataset were randomly chosen as training and testing data.

3. Specify the desired variable.

4.Create the Classifier using the training set as a foundation.

5.Train the classifier while reducing noise using real-time picture domain analysis.

6. Predict the testing set using the training dataset.

**Adaptive DWT**

Wavelets represent the signs which are essentially local in scale and time and by and large have an unpredictable shape. A waveform called a wavelet is a restricted length that has a typical worth of zero(0). The term 'wavelet' comes from the data that they are coordinated to zero; they wave all over across the axis. This feature guarantees that information isn't over-addressed. A sign can be disintegrated into various scaled and moving exhibitions of the first wavelet. Transformation of the wavelet can be utilized to break down a sign into part wavelets. Whenever this is done the coefficients of the wavelets can be demolished to eliminate a portion of the subtleties. Wavelets have the option to isolate the great subtleties in a sign. Lesser wavelets can be utilized to isolate an exceptionally fine subtlety in a sign, while large wavelets can recognize the Noise Elimination coarse subtleties. Furthermore, there are a lot more various wavelets to choose from. Many kinds of wavelets are Morlet, Daubechies, and so on. One specific wavelet might create a more indication of the sparse signal than another, so various types of wavelets should be inspected to see which is generally very much matched to picture compression

The benefits of the Novel Kalman Filter are, Increases in the exactness rate, Reserving the image and the series of time-low frequency exact signals, and being Adaptable for the images in real-time.

**Pseudo code**

input-Data for training and testing .

output-A category of information testing and accuracy .

1. A trained dataset has been used.

2. Calculated the predictor variables' infer and extensive deviation.

3.Continuously calculated using the Gauss-Density Equation the probability of the predictor variable. until all predictor variables' probabilities are computed.

4. Determine the probability for each class.

5. The highest likelihood was attained.

# 

# **STATISTICAL ANALYSIS**

Statistical software tool IBM SPSS with the standard version 26.0 to discover the value of SD (Standard Deviation), mean deviation data, significance point data and also drawing the graphical descriptions, etc. The SPSS tool was inclined in the present research process for investigating given data. Group statistics practice and self-determining sample tests were directed at the investigational outcomes and the graph Noise Elimination was created for two various graphs with two different types of features under the specific experimental stage.

Datasets for training and testing are selected for the database. The training dataset is established by reclaiming the test dataset from the real dataset as long as 400 images data as a whole.

**RESULTS**

MATLAB tool is used to examine the data and the accuracy value is assessed among Kalman and Adaptive DWT. For real-time datasets, the proposed Novel Kalman Filter offers an improved accuracy rate than the Adaptive DWT. The accuracy rate of the Novel Kalman Filter 90.13 % and the Adaptive DWT 89.35 % illustrates group statistics based on the real-time dataset of this current research work.

Table 1. Comparison of prediction of accuracy between novel kalman Filters and Adaptive DWT. The novel kalman Filters achieved an accuracy of 90.13% compared to Adaptive DWT having 89.35%. It shows that the novel kalman Filters performed significantly better than Adaptive DWT For Noise Detection and Removal in Real Time Images. The precision and execution of novel kalman filters were found to be significantly higher than those of Adaptive DWT.This indicates that novel kalman filters are a better choice than Adaptive DWT for this particular dataset and task.

Table 2 Group information displaying the mean, popular deviation, and fashionable error imply values for the two algorithms novel kalman filter and Adaptive DWT algorithm - with 10 sample sizes. The Performance of novel kalman filter and Adaptive DWT on the Noise Detection and Removal in Real Time Image Is implemented for the given dataset. The results show that the novel kalman filter has a standard deviation of 3.293 and a standard error mean of 1.041. For Adaptive DWT, with a standard deviation of 3.026 and a standard error mean of 0957.

Table 3 It shows the results of the 2-tailed significance test, which indicates that the difference in accuracy between the two algorithms is statistically insignificant. The 2-tailed significance value of less than 0.05 (p< 0.05) supports the hypothesis that the novel kalman filter is a better choice than Adaptive DWT for this dataset and task

**DISCUSSION**

The Adaptive DWT filter is used in the former research work, with a mean rate of accuracy of 87.90% . Novel Kalman Filter is designed, which has a mean accuracy rate of 91.60%.

The introduction of a method for removing unnecessary information from mechanical signs that relied on adaptive discrete wavelet separation and transformation [(Suneetha and Srinivasa Reddy 2021)](https://paperpile.com/c/ihOtTi/wQGw). The wavelet change's separated components were the input signals for the adaptive filtration after multi-scale disintegration [(Elmogy and Mahmoud 2017)](https://paperpile.com/c/ihOtTi/Emyx). It illustrates howNoise Elimination the method can effectively reduce irrelevant signals through the use of the reenacted signal. The suggested method for eliminating noise has been successfully used to identify faults in bearing signs . [(Jude Hemanth 2022)](https://paperpile.com/c/ihOtTi/jyVp)

One of the most essential and common assessment methods is the Novel Kalman Filter methodology[(S. Z. Li 2009)](https://paperpile.com/c/ihOtTi/8ZIF). It generates evaluations of hidden away aspects based on inaccurate and unreliable assumptions [(Gökcen and Kalyoncu 2020)](https://paperpile.com/c/ihOtTi/ZUIN). The Novel Kalman Filter also predicts the framework state in the future from prior evaluations [(Lukac et al. 2006)](https://paperpile.com/c/ihOtTi/kcsc). The filter bears Rudolf E. Kálmán's name [(Brereton 2018)](https://paperpile.com/c/ihOtTi/WMJk). Kálmán published his widely read paper in 1960 presenting a recursive solution to the discrete data linear sifting problem. Today, the Novel Kalman Filter is used in a wide range of applications, including target following (Radar), area and route frameworks, control frameworks, PC designs, and a lot more[(Science Abstracts: Electrical & Electronics Abstracts. Series B 1995)](https://paperpile.com/c/ihOtTi/SaCE). The Novel Kalman Filter

DWT, which is discovered to provide a rapid estimate of Wavelet Change and depends on sub-band coding.[FathimuthuJoharah S et al., 2017](http://www.ijirset.com/upload/2017/june/46_IJIRSET_Paper_Template%20_1_%20_2_%20_2_.pdf) indicates an examination of noise expulsion in an X-ray liver picture utilizing discrete wavelet change at the disintegration of the picture at level 1 and by channels[(Smolka, Malik, and Malik 2015)](https://paperpile.com/c/ihOtTi/fOA5) . The exhibition of removal of noise is assessed regarding PSNR, MSE, and accuracy rate [(HosseinKhani et al. 2018)](https://paperpile.com/c/ihOtTi/ZAe2)

**CONCLUSION**

In the image noise detection and removal, the proposed Novel Kalman Filters outperforms the existing adaptive dwt Filter in terms of accuracy (90.13% Vs 89.35%). From the simulation results and statistical analysis, the Novel Kalman Filters is recommended to use in the field of image processing for sensitive information .

# **DECLARATIONS**

**Conflicts of Interest**

The author declares no conflicts of interest.

# **Author’s contribution**

Author KD was involved in data collection, data analysis, and manuscript writing. Author GK was involved in conceptualization, data validation, and critical review of the manuscript.

# **Acknowledgement**

The authors would like to express their gratitude towards Saveetha School of Engineering and Saveetha Institute of Medical And Technical Sciences (formerly known as Saveetha University) for providing the necessary infrastructure to carry out this work successfully.

**Funding**

We thank the following organizations for providing financial support that enabled us to complete the research.

1. Sri cuba innovations pvt .ltd.
2. Saveetha School of Engineering
3. Saveetha University.
4. Saveetha Institute of Medical and Technical Sciences.

**REFERENCES**

[Brereton, Richard G. 2018. Chemometrics: Data Driven Extraction for Science. John Wiley & Sons.](http://paperpile.com/b/ihOtTi/WMJk)

[Elmogy, A. M., and E. Mahmoud. 2017. “Image Noise Detection and Removal Based on Enhanced gridLOF Algorithm.” International Journal of.](http://paperpile.com/b/ihOtTi/Emyx) <https://pdfs.semanticscholar.org/a2c7/3f68f38f33125fab7e348b60aea633de3f58.pdf>[.](http://paperpile.com/b/ihOtTi/Emyx)

[Ersboll, Bjarne K. 2007. Image Analysis: 15th Scandinavian Conference, SCIA 2007, Aalborg, Denmark, June 10-24, 2007, Proceedings. Springer Science & Business Media.](http://paperpile.com/b/ihOtTi/HhxT)

[Gökcen, Alpaslan, and Cem Kalyoncu. 2020. “Real-Time Impulse Noise Removal.” Journal of Real-Time Image Processing 17 (3): 459–69.](http://paperpile.com/b/ihOtTi/ZUIN)

[He, Huaiwu, Zhanqi Zhao, Knut Moeller, and Yun Long. 2022. Bedside Visual Image Technologies for Respiratory and Circulatory Management in Intensive Care Settings. Frontiers Media SA.](http://paperpile.com/b/ihOtTi/f7Cl)

[HosseinKhani, Zohreh, Mohsen Hajabdollahi, Nader Karimi, Reza Soroushmehr, Shahram Shirani, Kayvan Najarian, and Shadrokh Samavi. 2018. “Adaptive Real-Time Removal of Impulse Noise in Medical Images.” Journal of Medical Systems 42 (11): 216.](http://paperpile.com/b/ihOtTi/ZAe2)

[Jude Hemanth, D. 2022. Machine Learning Techniques for Smart City Applications: Trends and Solutions. Springer Nature.](http://paperpile.com/b/ihOtTi/jyVp)

[Li, Jianxin, Sen Wang, Shaowen Qin, Xue Li, and Shuliang Wang. 2019. Advanced Data Mining and Applications: 15th International Conference, ADMA 2019, Dalian, China, November 21–23, 2019, Proceedings. Springer Nature.](http://paperpile.com/b/ihOtTi/oUGh)

[Li, Stan Z. 2009. Encyclopedia of Biometrics: I - Z. Springer Science & Business Media.](http://paperpile.com/b/ihOtTi/8ZIF)

[Lukac, Rastislav, Bogdan Smolka, Konstantinos N. Plataniotis, and Anastasios N. Venetsanopoulos. 2006. “Vector Sigma Filters for Noise Detection and Removal in Color Images.” Journal of Visual Communication and Image Representation 17 (1): 1–26.](http://paperpile.com/b/ihOtTi/kcsc)

[Philips, Wilfried, Dan Popescu, and Paul Scheunders. 2007. Advanced Concepts for Intelligent Vision Systems: 9th International Conference, ACIVS 2007, Delft, The Netherlands, August 28-31, 2007, Proceedings. Springer.](http://paperpile.com/b/ihOtTi/WPEf)

[Science Abstracts: Electrical & Electronics Abstracts. Series B. 1995.](http://paperpile.com/b/ihOtTi/SaCE)

[Smolka, Bogdan, and Andrzej Chydzinski. 2005. “Fast Detection and Impulsive Noise Removal in Color Images.” Real-Time Imaging 11 (5): 389–402.](http://paperpile.com/b/ihOtTi/3Doe)

[Smolka, Bogdan, Krystyna Malik, and Dariusz Malik. 2015. “Adaptive Rank Weighted Switching Filter for Impulsive Noise Removal in Color Images.” Journal of Real-Time Image Processing 10 (2): 289–311.](http://paperpile.com/b/ihOtTi/fOA5)

[Suneetha, Akula, and E. Srinivasa Reddy. 2021. “Robust Gaussian Noise Detection and Removal in Color Images Using Modified Fuzzy Set Filter.” Journal of Intelligent Systems 30 (1): 240–57.](http://paperpile.com/b/ihOtTi/wQGw)

[Bouhlel, Med Salim, and Stefano Rovetta. 2019. Proceedings of the 8th International Conference on Sciences of Electronics, Technologies of Information and Telecommunications (SETITi 18), Vol.2. Springer](http://paperpile.com/b/ihOtTi/OCTe)

[Wen Tao Sui](https://www.researchgate.net/scientific-contributions/Wen-Tao-Sui-2013374649?_sg%5B0%5D=roA_qk0p2hLx-hDAhYiUKXTpBhI36VHlBopRKdu1YeaCndJjFnJB7yRHALOMWyA8MK0afFI.eUxKymYcvPPEqZCTMJGEuAfHvUjsOPHN0HPjFKBKRjM_9ZofYl-pFKZ1r_rUiIHNW-ll1bapftajAi4kA1WtPw&_sg%5B1%5D=PS8uErhf4dm1hwBNZGr_T0gBXTO1lG81E2HdxEH8a09OD7MgpOLAD0LXMAZgP2NQJy6WIEc.h-8tLehw8LJKhG0Xqh14mrAXcF9IvyEZRZVUwynP5T7XIMK5Wh8a5s5geOm88OKMY-YQcQDmB6hkWEKE9g6qBg)&[Dan Zhang](https://www.researchgate.net/scientific-contributions/Dan-Zhang-70125214?_sg%5B0%5D=roA_qk0p2hLx-hDAhYiUKXTpBhI36VHlBopRKdu1YeaCndJjFnJB7yRHALOMWyA8MK0afFI.eUxKymYcvPPEqZCTMJGEuAfHvUjsOPHN0HPjFKBKRjM_9ZofYl-pFKZ1r_rUiIHNW-ll1bapftajAi4kA1WtPw&_sg%5B1%5D=PS8uErhf4dm1hwBNZGr_T0gBXTO1lG81E2HdxEH8a09OD7MgpOLAD0LXMAZgP2NQJy6WIEc.h-8tLehw8LJKhG0Xqh14mrAXcF9IvyEZRZVUwynP5T7XIMK5Wh8a5s5geOm88OKMY-YQcQDmB6hkWEKE9g6qBg)(2010), “DWT-Based Adaptive Filter and its Application on Canceling Noise in Mechanical Signals”, June 2010, [Key Engineering Materials](https://www.researchgate.net/journal/Key-Engineering-Materials-1662-9795) 439-440:6-11, DOI: [10.4028/www.scientific.net/KEM.439-440.6](http://dx.doi.org/10.4028/www.scientific.net/KEM.439-440.6)

**TABLES AND FIGURES**

**Table 1**. Comparison of prediction of accuracy between novel kalman filter and Adaptive DWT. Novel kalman filter achieved an accuracy of 90.13% compared to the Adaptive DWT having 89.35%.


| **Sl.no** | **Novel kalman filter** | **Adaptive DWT** |
| --- | --- | --- |
| 1 | 90.13 | 89.35 |
| 2 | 89.45 | 88.16 |
| 3 | 88.59 | 87.95 |
| 4 | 87.54 | 86.96 |
| 5 | 86.91 | 85.86 |
| 6 | 85.54 | 84.75 |
| 7 | 84.48 | 83.49 |
| 8 | 83.94 | 82.84 |
| 9 | 82.91 | 81.93 |
| 10 | 81.53 | 80.18 |

**Table 2.** Mean, standard deviation, and standard error mean for, Novel Kalman Filter and adaptive dwt is given below..

| **Algorithm** | | **N** | **Mean** | **Standard Deviation** | **Standard Error Mean** |
| --- | --- | --- | --- | --- | --- |
| Accuracy | Kalaman filter | 10 | 90.13 | 3.293 | 1.041 |
| Adaptive DWT | 10 | 89.35 | 3.026 | 0.957 |

**Table 3.** An independent sample T-test is performed for the two groups for significance and standard error determination. The significance value p=0.005 (p<0.05) shows that two groups are statistically significant

|  | | **Levene’s test for equality of variables** | | **T-test for Equality of means** | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **F** | **Sig** | **t** | **df** | **Sig (2-tailed)** | **Mean Difference** | **Std. Error Difference** | **95% confidence interval of the Difference** | |
| **Lower** | **Upper** |
| **Accuracy** | Equal variances assumed | 0.169 | 0.685 | 0.549 | 18 | 0.005 | .776 | 1.414 | -2.195 | 3.747 |
| Equal variances not assumed |  |  | .549 | 17.874 | 0.005 | .776 | 1.414 | -2.197 | 3.749 |

****

**Graph**

**Fig. 1.**Comparison of the mean accuracy between the Novel Novel Kalman Filter and the adaptive dwt. The adaptive dwt's standard deviation is somewhat lower than the Novel Novel Kalman Filter, and its mean accuracy is higher than the latter. Adaptive dwt versus Novel Novel Kalman Filter on the X axis. Y Axis: Means Detection Accuracy ±1 SD.